**SpeedAC iQ – In Process V3.2.6 changes summary:**

***IMPORTANT: Databases from the previous versions are compatible***

**Fixes:**

* “0”s sometimes read in Additional Live Info in PLC

**Improvements/New features:**

* The Batch Target Weight can be changed via PLC
* The Batch Target Weight can be read via PLC – Additional Live Info
* The Throughput Weight can be read via PLC – Additional Live Info

**SpeedAC iQ – In Process V3.2.5 changes summary:**

***IMPORTANT: Databases from the previous versions are compatible***

**Improvements/New features:**

**Fixes:**

* New total weight is submitted after empty weight recorded;

**Improvements/New features:**

* The Target Weight can be changed via PLC;